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Annex B2 - Product environmental attributes
Computers and computer monitors

The declaration may be published only when all rows and/or fields marked with * are filled-in (n.a. for not applicable).

Additional information regarding each item may be found under P15.
	Brand *
	NEC
	Logo

	Company name *
	NEC Display Solutions, Ltd.

NEC Display Solutions Europe GmbH
	

	Contact information *
e-mail address
	m.utsunomiya@nec.com
Sebastian.Antoni@nec-displays.com
	

	Internet site *
	www.nec-display-solutions.com

	Additional information
	


	The company declares (based on product specification or test results based obtained from sample testing), that the product conforms to the statements given in this declaration.

	Type of product *
	Monitor

	Commercial name *
	MultiSync EA272F

	Model number *
	EA272F

	Issue date *
	2020-10-07

	Intended market *
	 FORMCHECKBOX 
 Global   FORMCHECKBOX 
 
 Asia, Pacific & Japan   Europe   Americas        Other   

	Additional information
	     


This is an uncontrolled copy when in printed form. Please refer to the contact information for the latest version.

	About Annex B2

Annex B2 reflects Product environmental attributes relevant for Computers and Computer Monitors. The following items from the ECMA‑370 Main body are not shown in the template:

P4.1 – P4.3 Consumable materials

P9.1 TEC and Print speed

P10.2 - P10.3 Chemical emissions from printing products 

P11.1 - P11.3 Consumable materials for printing products.


	Model number *
	EA272F
	Logo
	

	Issue date *
	2020/10/07
	
	


	Product environmental attributes - Legal requirements

Requirement met


	Item
	
	Yes
	No
	n.a.

	P1
	Hazardous substances and preparations
	

	P1.1*
	Products do comply with current European RoHS Directive. (See legal reference and NOTE B1) 
	 FORMCHECKBOX 

	
	

	P1.2*
	Products do not contain Asbestos (see legal reference). 

Comment: Legal reference has no maximum concentration value.     
	 FORMCHECKBOX 

	
	

	P1.3*
	Products do not contain Ozone Depleting Substances: Chlorofluorocarbons (CFC), hydrobromofluorocarbons (HBFC), hydrochlorofluorcarbons (HCFC), Halons, carbontetrachloride, 1,1,1-trichloroethane, methyl bromide (see legal reference). Comment: Legal reference has no maximum concentration values.     
	 FORMCHECKBOX 

	
	

	P1.4*
	Products do not contain more than; 0,005% polychlorinated biphenyl (PCB), 0,005% polychlorinated terphenyl (PCT) in preparations (see legal reference).
	 FORMCHECKBOX 

	
	

	P1.5*
	Products do not contain more than 0,1% short chain chloroparaffins (SCCP) with 10-13 carbon atoms in the chain containing at least 48% per mass of chlorine in the SCCP (see legal reference).
	 FORMCHECKBOX 

	
	

	P1.6*
	Parts with direct and prolonged skin contact do not release nickel in concentrations above 0,5 (g/cm2/week (see legal reference). 

Comment: Max limit in legal reference when tested according to EN1811:2011-5.  
	 FORMCHECKBOX 

	
	 FORMCHECKBOX 


	P1.7*
	REACH Article 33 information about substances in articles is available at (add URL or mail contact):

	 FORMCHECKBOX 

	
	


	P2
	Batteries
	

	P2.1*
	If the product contains a battery or an accumulator, the battery/accumulator is labeled with the disposal symbol. Information on proper disposal is provided in user manual. (See legal reference)
	
	
	 FORMCHECKBOX 


	P2.2*
	Batteries or accumulators do not contain more than 0,0005% of mercury or 0,002% of cadmium. (See legal reference)
	
	
	 FORMCHECKBOX 


	P2.3*
	Batteries and accumulators are readily removable. (See legal reference)
	
	
	 FORMCHECKBOX 


	P2.4*
	Documentation includes the number of cycles the (secondary) battery can withstand. (See legal reference)
	
	
	 FORMCHECKBOX 


	P2.5*
	When internal batteries of a notebook computer cannot be “accessed and replaced by a nonprofessional user”, the related text is present and legible on the external packaging (see legal reference)
	
	
	 FORMCHECKBOX 


	P3
	Conformity verification & Eco design (ErP)
	
	
	

	P3.1*
	The product is CE-marked to show conformance with applicable legal requirements (see legal reference). 

The Declaration of Conformity can be requested at (add link or e-mail address):      
	 FORMCHECKBOX 

	
	

	P3.2*
	The product complies with the applicable Eco design requirements for energy-related products, 
(see legal reference).
	 FORMCHECKBOX 

	
	

	
	Required information is;
 FORMCHECKBOX 
 given in item P15 or added to this document, 



 available at (add URL):  
	
	
	 FORMCHECKBOX 


	P5
	Product packaging
	
	
	

	P5.1*
	Packaging and packaging components do not contain more than 0,01% lead, mercury, cadmium and hexavalent chromium by weight of these together.  
	 FORMCHECKBOX 

	
	

	P5.2*
	The packaging materials are marked with abbreviations and numbers indicating the nature of the material(s) used (see legal reference).
	 FORMCHECKBOX 

	
	

	P5.3*
	The product packaging material is free from ozone depleting substances as specified in the Montreal Protocol (see legal reference).

Comment: Legal reference has no maximum concentration values.
	 FORMCHECKBOX 

	
	

	P6
	Treatment information
	

	P6.1*
	Information for recyclers/treatment facilities is available (see legal reference).
	  FORMCHECKBOX 

	
	 FORMCHECKBOX 



	Model number *
	EA272F
	Logo
	

	Issue date *
	2020/10/07
	
	


	Product environmental attributes - Market requirements (See General NOTE GN below)
               - Environmental conscious design
Requirement met


	Item
	*=mandatory to fill in. Additional information regarding each item may be found under P14.
	Yes
	No
	n.a.

	P7
	Design
	

	
	Disassembly, recycling
	

	P7.1*
	Parts that have to be treated separately are easily separable
	 FORMCHECKBOX 

	
	

	P7.2*
	Plastic materials in covers/housing have no surface coating.
	 FORMCHECKBOX 

	
	

	P7.3*
	Plastic parts > 100 g consist of one material or of easily separable materials.
	 FORMCHECKBOX 

	
	

	P7.4*
	Plastic parts > 25 g have material codes according to ISO 11469 referring ISO 1043-4.
	 FORMCHECKBOX 

	
	

	P7.5
	Plastic parts are free from metal inlays or have inlays that can be removed with commonly available tools.
	 FORMCHECKBOX 

	
	

	P7.6*
	Labels are easily separable. (This requirement does not apply to safety/regulatory labels).
	 FORMCHECKBOX 

	
	

	
	Product lifetime
	

	P7.7*
	Upgrading can be done e.g. with processor, memory, cards or drives
	
	
	 FORMCHECKBOX 


	P7.8*
	Upgrading can be done using commonly available tools
	
	
	 FORMCHECKBOX 


	P7.9
	Spare parts are available after end of production for: 5 years
	
	
	

	P7.10
	Service is available after end of production for: 5 years
	
	
	

	
	Material and substance requirements
	

	P7.11*
	Product cover/housing material type (e.g. plastics, metal, aluminum):
	

	
	Material type: PC+ABS  
	Material type: 
	Material type: 
	

	P7.12
	Insulation materials of external electrical cables are PVC free. 
	
	 FORMCHECKBOX 

	

	P7.13
	Insulation materials of internal electrical cables are PVC free. 
	
	 FORMCHECKBOX 

	

	P7.14
	External plastic casing/cover parts > 25 g contain no more than 0,1% weight (1000 ppm) bromine and 0,1% weight (1000 ppm) chlorine attributable to brominated flame retardants, chlorinated flame retardants, and polyvinyl chloride or 0,3% weight (3000 ppm) bromine and 0,3% weight (3000 ppm) chlorine in parts containing more than 25% post-consumer recycled content.


	 FORMCHECKBOX 

	
	

	P7.15
	Printed circuit boards, PCBs (without components) are low halogen: all  FORMCHECKBOX 
 PCBs > 25 g  are low halogen as defined in IEC 61249-2-21. (See 
NOTE B2)

	
	 FORMCHECKBOX 

	

	P7.16
	Flame retarded plastic parts > 25 g in covers / housings are marked according ISO 1043-4:

Marking: >PC+ABS-FR(40)<
	 FORMCHECKBOX 

	
	

	P7.17
	Alt. 1: Chemical specifications of flame retardants in printed circuit boards > 25 g (without components):

TBBPA (additive)  
, TBBPA (reactive)  (See NOTE B3), Other; chemical name: 
Alt. 2: Chemical specifications of flame retardants in printed circuit boards (without components) > 25 g according ISO 1043-4: FR(16)

	 FORMCHECKBOX 

 FORMCHECKBOX 

	

	 FORMCHECKBOX 



	P7.18
	Alt. 1: Flame retarded plastic parts > 25 g contain the following flame retardant substances/preparations in concentrations above 0,1%:

1. C Chemical name: Bisphenol diphenyl phosphate, CAS #: 181028-79-5 (See NOTE B4)
2. Chemical name: 
3. Chemical name: 
Alt. 2: Chemical specifications of flame retardants in plastic parts > 25 g according ISO 1043-4: FR(40)
	 FORMCHECKBOX 

 FORMCHECKBOX 

	

	


	P7.19 
	In plastic parts > 25 g, flame retardant substances/preparations above 0,1% are used which have been assigned the following Risk phrases; 
The source(s) for these classifications is/are found at (add URL(s)): 

	

	 FORMCHECKBOX 


	 FORMCHECKBOX 




	Model number *
	EA242F
	Logo
	

	Issue date *
	2020/10/07
	
	


	Product environmental attributes - Market requirements (continued)
Requirement met

	Item
	
	Yes
	No
	n.a.

	
	Material and substance requirements (continued)

	P7.20*
	Postconsumer recycled plastic material content is used in the product (See NOTE B6):
 
If YES; at least one of the two alternatives below shall be answered;

a) Of total plastic parts’ weight > 25 g, the postconsumer recycled plastic material content (calculated as a percentage of total plastic by weight) is 
or

b) The weight of recycled material is 
	

	 FORMCHECKBOX 


	


	P7.21*
	Biobased plastic material content is used in the product (See NOTE B7):

If YES; at least one of the two alternatives below shall be answered;

a) Of total plastic parts’ weight > 25 g, the biobased plastic material content (calculated as a percentage of total plastic by weight) is      %. 

or

b) The weight of the biobased plastic material is      g.
	
	 FORMCHECKBOX 

	

	P7.22*
	Light sources are free from mercury, i.e. less than 0,1 mg/lamp.

If mercury is used specify: Number of lamps: 
	 FORMCHECKBOX 

	
	

	P7.23*
	If product includes an integral display, the total mercury content in the integrated display: 0mg
	 FORMCHECKBOX 

	
	 

	P8
	Batteries

	P8.1*
	Battery chemical composition: 
	
	
	 FORMCHECKBOX 


	P9
	Energy consumption (See NOTE B8)
	
	
	

	P9.1
	For the product the following power levels or energy consumptions are reported: 
	
	
	

	Energy mode *
	Power level at 
100 V AC
	Power level at
115 V AC
	Power level at
230 V AC
	Reference/Standard for energy modes and test method *
	

	EPS No-load
(External power supply / charger plugged in the wall outlet but disconnected from the product.)
	NA
	NA
	NA
	NA
	

	PTEC *
Typical Energy Consumption
	NA
	NA
	NA
	NA 
	 FORMCHECKBOX 


	ETEC *
Annual Energy Consumption
	NA    
	54.78 kWh/year
	52.11kWh/year
	Energy Star 8.0
	

	External Power Supply Efficiency Level (International Efficiency Marking Protocol) * : 
	

	 FORMCHECKBOX 


	Display resolution *
: 2.07 megapixels
	1920 x 1080 pixels
	

	Default time to enter energy save mode: 0.2 minutes 
	

	

	P9.2*
	Information about the energy save function is provided with the product. 
	 FORMCHECKBOX 

	
	

	P9.3
	Energy efficiency class (monitors only): A++
	
	
	
	


	Model number *
	EA242F
	Logo
	

	Issue date *
	2020/10/07
	
	


	Product environmental attributes - Market requirements (continued) 
Requirement met

	Item
	
	Yes
	No
	n.a.

	P10
	Emissions
	
	
	

	
	Noise emission – Declared according to ISO 9296 (See NOTE B9)
	
	
	

	P10.1 
	Mode 
	Mode description 


	Statistical upper limit A‑weighted sound power level, 
LWA,c (B)
	

	
	
	
	
	

	
	Idle 
	*

	* 
	 FORMCHECKBOX 


	
	Operation
	*

	* 
	 FORMCHECKBOX 


	
	Other mode
	

	  
	

	
	Measured according to:   ECMA-74  ISO 7779 
  Other 
	

	
	Electromagnetic emissions

	P10.4
	Computer display meets the requirement for low frequency electromagnetic fields of the following voluntary program(s):      
	
	
	 FORMCHECKBOX 


	P12
	Ergonomics for computing products 

	P12.1*
	The display meets the ergonomic requirements of ISO 9241-307 for visual display technologies.
	 FORMCHECKBOX 

	
	

	P12.2*
	The physical input device meets the requirements of ISO 9995 and ISO 9241-410. 
	
	
	 FORMCHECKBOX 


	P13
	Packaging and documentation 

	P13.1*
	Product packaging material type(s): Paper 
weight (kg): 1.255
Product packaging material type(s): EPS
weight (kg): 0.6
Product packaging material type(s): PE+EPE 
weight (kg): 0.035
	
	
	

	P13.2*
	Product plastic primary packaging is free from PVC. 
	 FORMCHECKBOX 

	
	

	P13.3*
	For product primary corrugated fiberboard packaging, specify the contained percentage of minimum post-consumer recovered fiber content: 90%
	
	
	

	P13.4*
	Specify media for user and product documentation (tick box): 
Electronic
  FORMCHECKBOX 
, Paper  FORMCHECKBOX 
, Other      


	
	
	

	P13.5
	(Please only complete this item if paper documentation used)
User and product documentation on paper media is chlorine-free:
If Yes, please specify:
	 FORMCHECKBOX 

	

	

	
	Totally chlorine-free 
	 FORMCHECKBOX 

	
	

	
	Elemental chlorine-free
	
	
	

	
	Processed chlorine-free
	
	

	

	P14
	Voluntary programs

	P14.1
	The product meets the requirements of the following voluntary program(s):


	
	ENERGY STAR®
	Criteria version: 8.0
	Date: 2020.8.7
	Product category: Display

	
	Eco-label:
 
	Criteria version: 
	Date: 
	Product category: 

	
	Eco-label:
 
	Criteria version: 
	Date: 
	Product category: 

	P15
	Additional information (See NOTE B10)

	P9
	Energy consumption of computer products; description of the tested product configuration:       

	     
	     

	     
	     

	     
	     


Legal references Europe Annex B2
	Reference
	Declaration item

	Directive 2011/65/EU (RoHS Directive)*
* Specific exemptions apply for certain products and applications.
	P1.1, P3.1

	Regulation (EC) 1907/2006 (REACH Regulation), annex XVII
	P1.2, P1.4, P1.6, P1.7 

	Regulation (EC) 2037/2000, 2038/2000, 2039/2000 (Marketing and use of Ozone layer depleting substances)
	P1.3, P5.3

	Norwegian regulation relating to restrictions on the use of certain dangerous chemicals 20.12.2002
	P1.5

	Directive 2006/66/EC (Battery and accumulators Directive), as amended.*
* These provisions shall not apply where, for safety, performance, medical or data integrity reasons, continuity of power supply is necessary and requires a permanent connection between the appliance and the battery or accumulator.
	P2.1, P2.2, P2,3, P8.1

	Directive 2014/35/EU (Low Voltage Directive)
	P3.1

	Directive 2014/30/EU (EMC Directive)
	P3.1

	Directive 2014/53/EU (RE Directive)
	P3.1

	Regulation (EC) 801/2013 amending Regulation (EC) No 1275/2008 with regard to ecodesign requirements for standby, off mode electric power consumption of electrical and electronic household and office equipment, and amending Regulation (EC) No 642/2009 with regard to ecodesign requirements for televisions 
	P3.1, P3.2

	Commission Regulation (EC) No 278/2009 of 6 April 2009 implementing Directive 2005/32/EC of the European Parliament and of the Council with regard to ecodesign requirements for no-load condition electric power demand and average active efficiency of external power supplies
	P3.1, P3.2, P9.1

	COMMISSION REGULATION (EU) No 617/2013 of 26 June 2013 implementing Directive 2009/125/EC of the European Parliament and of the Council with regard to ecodesign requirements for computers and computer servers
	P2.4, P2.5, P3.1, P3.2, P7.23, P9.1

	Regulation（EC）No 1272/2008 (CLP Regulation)
	P7.19

	Directive 2004/12/EC (Packaging Directive)
	P5.1

	Decision 97/129/EC (Secondary packaging legislation)
	P5.2

	Directive 2012/19/EU (WEEE directive)

Implementing Regulation (EU) 2019/290 establishing the format for registration and reporting of producers of electrical and electronic equipment to the register.

Commission Implementing Regulation 2017/699 establishing a common methodology for the calculation of the weight of electrical and electronic equipment (EEE) placed on the national market in each Member State and a common methodology for the calculation of the quantity of waste electrical and electronic equipment (WEEE) generated by weight in each Member State.
	P6.1


NOTE B1	 Restriction applies to the homogeneous material, unless other specified and expressed in weight %. Stating “Yes” means that the product is compliant with the mandatory requirements.


GENERAL NOTE	 Standard references should direct to the latest version of a standard. If an older version of a standard is used, section P15 shall be used for explanation.


NOTE B2	IEC 61249-2-21 defines maximum limits of 900 ppm for each of the substances chlorine and bromine and a maximum limit of 1500ppm of these substances combined. The standard does not address fluorine, iodine and astatine which are included in the group of halogens. 


NOTE B3 and B4	A Guidance document on Chemical substances is available; see ��HYPERLINK "http://www.ecma-international.org/publications/standards/Ecma-370.htm"�http://www.ecma-international.org/publications/standards/Ecma-370.htm�.


NOTE B5	If a certain substance has been assigned a certain risk phrases / hazard statement in the referenced source, this does not necessarily mean the substance has been tested for all of the hazards referred to by a certain customer.


NOTE B6	Applies to a product containing plastic parts whose combined weight exceeds 100 g with the exception of printed circuit boards, cables, connectors and electronic components and bio-based plastic material.


NOTE B7	The following is to be excluded from the calculation of percentage: printed circuit boards, labels, cables, connectors and electronic components and postconsumer recycled plastic


NOTE B8	A Guidance document on Energy Efficiency is available; �see �HYPERLINK "http://www.ecma-international.org/publications/standards/Ecma-370.htm"�http://www.ecma-international.org/publications/standards/Ecma-370.htm�.


NOTE B9	A Guidance document on Acoustic Noise is available; �see �HYPERLINK "http://www.ecma-international.org/publications/standards/Ecma-370.htm"�http://www.ecma-international.org/publications/standards/Ecma-370.htm�.





NOTE B10	Additional lines may be inserted to declare further items, by positioning the cursor at the far right of the row and hitting the <Enter> key.
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