# CUSTOM SIZE REGISTRATION (BYPASS)

Paper tray and paper type settings are explained in this section.
If you frequently use a non-standard size paper in the bypass tray, register that paper size in advance.
Registering the paper size saves you the trouble of setting the size each time you need to use it.
Up to three paper sizes can be registered.
Tap the key ([Custom 1] to [Custom 7]) in which you wish to register or change a paper size, and the registration screen appears.
Select whether you wish to enter the size in mm ("Size Input-AB") or inches ("Size Input-Inch"), and then set the X and Y dimensions of the paper.
"Size Input-AB"
The X direction can be set between 140 mm (or 148 mm if finisher installed) and 432 mm. The factory default setting is 420 mm.
The Y direction can be set between 90 mm and 297 mm. The factory default setting is 297 mm.
"Size Input-Inch"
The X direction can be set between 5-1/2" (or 5-7/8" if finisher installed) and 17". The factory default setting is 17".
The Y direction can be set between 3-5/8" and 11-5/8". The factory default setting is 11".
Back to top