# CLEANING THE PT CHARGER OF THE FIRST TRANSFER BELT

## Overview

If black or coloured lines appear even after you have cleaned the document glass, automatic document feeder, and main charger, clean the PT charger using the PT charger cleaner.

## Operation

Open the front cover.
Move the lock of the toner collection container to the release position, push it down until the toner collection container stops, and then slowly lift it up to remove it.
Clean the PT charger.
Gently pull out the PT charger cleaner to the position you feel appropriate, and then push it all the way in.
Repeat this operation three times.
Push the toner collection container into the machine.
Push the box in until it clicks into place.
Lock the toner collection container.
Move the toner collection container lock to the lock position.
Close the front cover.
Back to top