# LIST OF SETTING MODE FOR FAX

The following lists the Setting mode for fax and factory default settings.
Depending on the machine specifications and peripheral devices installed, it may not be possible to use some settings.
SYSTEM SETTINGS
U: General user; A: System administrator/Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| System Settings
| Yes | Yes
| F-Code Memory Box
| - | Yes | Yes
| Fax Data Receive/Forward - Fax Functions
| Yes | Yes
| Fax Settings
| Yes | Yes
| Receive Settings
| Auto Reception | Yes | Yes
| Multiple Set Print
| Disabled | Yes | Yes
| Staple *1
| Disabled | Yes | Yes
| Forward Received Data
| - | Yes | Yes
| Image Send Settings - Fax Functions
| No | Yes
| Fax Settings
| No | Yes
| Fax Default Settings
| No | Yes
| Dial Mode Setting
| Tone | No | Yes
| Auto Wake Up Print
| Enabled | No | Yes
| Pause Time Setting
| Varies depending on the machine configuration | No | Yes
| Fax Dest. Confirmation Mode
| Disabled | No | Yes
| Speaker Settings
| No | Yes
| Speaker
| Volume: 5 | No | Yes
| Ringer Volume
| Volume: 5 | No | Yes
| Line Monitor
| Volume: No Sound | No | Yes
| Fax Receive Complete Signal
| Volume: 5; Tone Pattern: 3 Transmission Complete Sound Time Setting: 3 sec. | No | Yes
| Fax Send Complete Signal
| Volume: 5; Tone Pattern: 3 Transmission Complete Sound Time Setting: 3 sec. | No | Yes
| Fax Communication Error Signal
| Volume: 5; Tone Pattern: 3 Transmission Complete Sound Time Setting: 0.3 sec. each | No | Yes
| Remote Reception Number Setting
| 5 | No | Yes
| Original Print on Transaction Report
| Print Out Error Report Only | No | Yes
| Transaction Report Print Select Setting
| No | Yes
| Single Sending
| Print Out Error Report Only | No | Yes
| Broadcasting
| Print Out All Report | No | Yes
| Receiving
| Do not Print | No | Yes
| Confidential Reception
| Print Out Notice Page | No | Yes
| Activity Report Print Select Setting
| No | Yes
| Auto Print at Memory Full
| Disabled | No | Yes
| Print Daily at Designated Time
| Disabled | No | Yes
| ECM
| Enabled | No | Yes
| Digital Subscriber Network
| Disabled | No | Yes
| DRD(Distinctive Ring Detection)
| Disabled | No | Yes
| Fax Send Settings
| No | Yes
| Auto Reduction Sending Setting
| Enabled | No | Yes
| Rotation Sending Setting
| All Enabled | No | Yes
| Quick On Line Sending
| Enabled | No | Yes
| Printing Page Number at Receiver
| Enabled | No | Yes
| Sender/Destination Name Change
| Fax No. | No | Yes
| Date/Own Number Print Position Setting
| Outside the Original Image | No | Yes
| Recall in Case of Line Busy
| See "Country Differentiation Table" | No | Yes
| Recall in Case of Communication Error
| See "Country Differentiation Table" | No | Yes
| Prohibit Fax Broadcasting
| Disabled | No | Yes
| Fax Receive Settings
| No | Yes
| Number of Calls in Auto Reception
| 2 times | No | Yes
| Switching from Manual to Automatic Reception *2
| Disabled | No | Yes
| Duplex Reception Setting
| Disabled | No | Yes
| Auto Receive Reduce Setting
| Enabled | No | Yes
| Print Style Setting
| Auto Size Select | No | Yes
| Set the Telephone Number for Data Forwarding
| - | No | Yes
| Letter Size RX Reduce Print *2
| Disabled | No | Yes
| Receiving Date & Time Print
| Disabled | No | Yes
| A3 RX Reduce
| Disabled | No | Yes
| Fax Output Settings
| Varies depending on the machine configuration | No | Yes
| Number of Prints
| 1 | No | Yes
| Staple Settings*1
| 1 Staple at Back | No | Yes
| Paper Size
| A4 or A3 (8-1/2 x 11 or 8-1/2 x 11R) | No | Yes
| Allow/Reject Number Setting
| No | Yes
| Allow/Reject Number Setting
| All Disabled | No | Yes
| Reject Unknown Calls
| Disabled | No | Yes
| Fax Polling Security
| No | Yes
| Set Fax Polling Security
| Enabled | No | Yes

*1 When a saddle finisher or finisher is installed
*2 This function is not available in some countries and regions.
Back to top