# WIRELESS SETTINGS

It provides access to a network via a wireless LAN.
Clicking the [Submit] button stores the settings.
Wireless Settings
Used to enable or disable the wireless LAN and show the status of wireless LAN.
Connection Type Switching
Switches between infrastructure mode and access point mode to match the wireless LAN environment that is used.
Current Setting
Shows settings, such as the SSID of a wireless LAN and security type. If the wireless LAN is disabled, "--" appears.
Current Wireless Status
This shows reception levels (Max. 100) of the wireless LAN and IP addresses.
Show Wireless Setting Screen
Click the [Setup] button.
In the Wireless Setting screen, you can configure the SSID of a wireless LAN, Security Type, Encry., and Security Key.
Initialize Wireless Settings
Click the [Initialize] button.
The settings for SSID, Security Type, Encry., and Security Key are initialized.
Wireless Setting screen
Configure the SSID of a wireless LAN, Security Type, Encry., and Security Key.
Clicking the [Submit] button stores the settings.
SSID
Enter an SSID using up to 32 characters.
Security Type
Select a security type.
Encry.
Select an encryption type.
Security Key
Enter a security key.

Security Type | Security Key
--- | ---
WEP 64bit | 5 characters or 10-digit hexadecimal number
WEP 128bit | 13 characters or 26-digit hexadecimal number
WAP/WAP2 | 8 to 63 characters or 64-digit hexadecimal number

Show Security Key
If it is set to ON, the security key appears.
Device IP Address
Use this setting for the access point mode. Enter the IP address.
Channel to Be Used
Use this setting for the access point mode. Select the channel to be used in wireless LAN.
Sending Output
Use this setting for the access point mode. Configure the sending output.
Bandwidth
Use this setting when the communication mode is "11n" in access point mode. Select the bandwidth to be used.
IP Address Distribution Range Setting
Use this setting for the access point mode. Configure the range to be used the IP address.
Back to top