# PRINTING AND SENDING SIMULTANEOUSLY

## Overview

This function prints data created in an application from the machine and simultaneously sends the data to the addresses stored in the machine.
This function allows you to complete two tasks, printing and sending, with one operation from the printer driver.

- Addresses must be stored in advance in the machine. For more information, see "STORING ADDRESSES THROUGH DIRECT ENTRY" and " STORING ADDRESSES THROUGH GLOBAL ADDRESS SEARCH".
- You must complete the preparatory steps for using each sending function of the machine. For more information, see the explanation of each sending function.

- This function is available in a Windows environment.
- This function can be used when the SPDL2-c printer driver is used.
- You cannot print and send data simultaneously when [System Settings] in "Setting mode" → [Printer Settings]→[Default Settings]→[Prohibit utilize sending function at print] is selected.

## Operation

Windows
Click the [Job Handling] tab and click the [Print and Send] button.
Select the [Print and Send] checkbox so that the checkmark appears.
Click the [Get Address Book] button.
From the "Address Book" list, select the address to which you wish to send the data, and click the [Add] button to add the address to the "Destination" list.

- If you wish to send the data to all addresses, click the [Add All] button.
- To delete an address from the "Destination" list, select the address and click the [Delete] button. If you wish to delete all addresses, click the [Delete All] button.

Up to 50 destinations can be specified.
Click the [OK] button.
The printer driver settings are applied to sending settings.
Back to top