# RECEIVING A FAX AFTER ANSWERING A CALL ON THE EXTENSION TELEPHONE(REMOTE RECEPTION)

## Overview

Follow the steps below if you need to start fax reception after answering a call and speaking on the extension telephone.
If you are using a pulse line, set the extension to send tone signals.

- To receive a fax after answering a call on the extension telephone:
  In "Setting mode", select [System Settings]→[Fax Data Receive/Forward]→[Fax Settings]→[Receive Settings] to enable [Manual Reception].
- To change the number to receive faxes:
  In "Setting mode", select [System Settings]→[Image Send Settings]→[Fax Settings]→[Default Settings]→[Remote Reception Number Setting].

## Operation

While the machine is ringing, pick up the receiver to speak.
Signal the machine to start fax reception.
Press from the extension telephone.
Replace the receiver.
The machine beeps when reception ends.
Back to top