# INSERTING INSERTION SHEETS IN BETWEEN TRANSPARENCY FILMS(TRANSPARENCY INSERTS)

## Overview

When copying on transparency film, the sheets may stick together due to static electricity.
The transparency inserts function can be used to automatically insert a sheet of paper between each sheet of transparency film, making the sheets easy to handle.
It is also possible to copy on insertion sheets.
When performing 2-sided copying, only "2-side to 1-side" mode can be used.

- The number of copies cannot be selected in this mode.
- Transparency film can only be placed in the bypass tray.

## Operation

Place the transparency film face down in the bypass tray, and load transparency film sheets.
After loading the transparency film, configure the bypass tray settings.

- MAKING COPIES USING THE BYPASS TRAY

Place the original and tap the [Preview] key.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Tap the [Others] key, and tap the [Transparency Inserts] key.
Tap the [On] key.
When making a copy on insertion sheets, tap the [Also Make Copy on Inserts] checkbox to set to .
After the settings are completed, tap and [Back] keys in sequence.
To cancel the transparency inserts setting:
Tap the [Off] key.
Check the preview image in the preview screen.
Check whether or not settings produce the required results.
To cancel all settings:
Tap the [CA] key.
Tap the [Colour Start] or [B/W Start] key to start copying.
When making only one set of copies, you do not need to specify the number of copies.
To make two or more sets of copies:
Tap the copies display key to specify the number of copies.
Back to top