# THE TRANSMITTED FAX IS REDUCED BY THE RECEIVING FAX MACHINE

If you are unable to solve a problem using the solutions in this manual, press the [Power] button and then turn the main power switch to the ""position. Wait at least 10 seconds and then turn the main power switch to the ""position. After the main power indicator colour changes to green, press the [POWER] button.
When the background colour of the job status display at the upper right corner of the touch panel is not grey, do not switch off the main power switch or unplug the power plug. This may damage the hard drive or cause the data being stored or received to be lost.

Point to check | Solution
--- | ---
Has the rotation sending been set? | Enable "Rotation Sending Setting" before transmission. When [Rotation Sending Setting] is not enabled (the image is not rotated), an original placed in the vertical orientation may be reduced by the receiving machine. "Setting mode" → [System Settings]→[Image Send Settings]→[Fax Settings]→[Send Settings]→[Rotation Sending Setting] If "Mixed Size Original" is enabled in Others and an original with a different width is sent, rotate transmission will be disabled.

Back to top