# COPY SETTINGS

The following settings are related to copying.
Default settings selected with these settings apply to all functions of the machine (not just the copy function).
Copy Exposure Adjustment
Adjusts the exposure level when [Auto] is used for the copy exposure.
Colour
Sets the copy exposure level in colour mode for the document glass and for the automatic document feeder.
B/W
Sets the copy exposure level in black & white mode for the document glass and for the automatic document feeder.
Rotation Copy Setting
When the original and paper are placed in different orientations, this function automatically rotates the image 90 degrees to enable correct copying on the paper.
Enable the Rotation Copy setting to copy an A5 (5-1/2" x 8-1/2") size original on A5R (5-1/2" x 8-1/2"R) paper.
Add or Change Extra Preset Ratios
Add two enlargement preset ratio values (101% to 400%) and two reduction preset ratio values (25% to 99%).
Also, you can change the preset ratio if necessary.
Preset ratios other than added preset ratios cannot be changed.
Setting a Maximum Number of Copies
This is used to set the maximum number that can be entered for the number of copies (number of continuous copies). Any number from 1 to 999 can be specified.
Initial Margin Shift Setting
This is used to set the default margin shift amount. Specify a value from 0 mm (0") to 50 mm (2") in increments of 3 mm (1/8") for both the front and reverse sides.
Erase Width Adjustment
This is used to set the default erase width for erase function. Specify a value from 0 mm (0") to 25 mm (1") in increments of 3 mm (1/8") for both edge erase and centre erase.
Initial Multi Shot Setting
Set the default state for Multi Shot. Select the page layout for Multi Shot, whether or not borders are added, and if added, whether the borders are solid lines or dotted lines.
Card Shot Settings
This is used to set the default original size for the card shot function.
Specify a value from 25 mm (1") to 216 mm (8-1/2") in increments of 3 mm (1/8") for both the X (horizontal) and Y (vertical) dimensions of the original.
Fit to Page
Enable this setting to have the [Fit to Page] key always appear in the card shot screen.
Automatic Saddle Stitch
Saddle stitch stapling take place automatically when the pamphlet copy function is used.
Initial Tab Copy Setting
This is used to set the default image shift width (tab width) for tab copying.
Specify a value from 0 mm (0") to 25 mm (1") in increments of 3 mm (1/8").
Disabling of Registration/Deletion of Program
This is used to prohibit the deletion and changing of copy settings stored in job programs.
Disabling of Bypass-Tray in Duplex Copy
Disables the use of the bypass tray when making 2-sided copies.
The bypass tray is often used to feed label sheets, transparency film, and other special media for which 2-sided copying is prohibited. If a sheet of one of these special media enters the reversing unit, a misfeed or damage to the unit may result. If special media for which 2-sided copying is prohibited is often used, it is recommended that you enable this setting.
Disabling of Auto Paper Selection
Disables the Auto Paper Selection function.
When this setting is enabled, automatic selection of paper that is the same size as the original on the document glass or in the automatic document feeder does not take place.
Auto Selection Setting of Tray that is Supplied the Paper
When this setting is enabled and paper is loaded into a tray while the machine is on standby in copy mode, that tray is automatically selected.
Disabling Registration of Custom Image
Disables storage of a custom image.
Disabling sending while copying
Disables the Image Send function during copy.
B/W 600 dpi x 600 dpi Scanning Mode for Document Feeder
The resolution for copying in black and white using the automatic document feeder can be changed from 600 x 400 dpi to 600 x 600 dpi (high quality mode).
When high quality mode is used, fine print and thin lines are reproduced with greater clarity, however, the scanning speed is slower.
When high quality mode is not selected, the following conditions must be satisfied in order to scan at 600 x 400 dpi and attain the fastest speed.

- The copy ratio must be set to 100%.
- Do not select a special mode that will change the ratio.
- [Copy of Copy] must not be enabled.
- Do not copy in black and white with the [Colour Start] key.

B/W Quick Scan from Document Glass
The resolution for copying in black and white using the document glass can be changed from 600 x 600 dpi to 600 x 300 dpi (high speed mode).
When high speed mode is selected, the first copy time is quicker, however, the copy image is not as clear.
When high quality mode is not selected, the following conditions must be satisfied in order to scan at 600 x 300 dpi and attain the fastest speed.

- The copy ratio must be set to 100%.
- Do not select a special mode that will change the ratio.
- [Copy of Copy] must not be enabled.
- Do not copy in black and white with the [Colour Start] key.

Auto Clear Before Copy Job
Enables the Auto Clear function during copy even when a copy job is not completed. This protects the machine from being held due to the incomplete copy job.
Back to top