# FORWARDING RECEIVED DATA MANUALLY

## Overview

Received faxes can be forwarded manually after receipt.
This function is available when [System Settings]→[Operation Settings]→[Preview Setting]→[Received Data Image Check Setting] is enabled* in "Setting mode".
* The factory default setting is disabled.

## Operation

When data is received, is shown at the top of the screen.

1. #### In the System Information, tap the [Event Information] tab and tap the [Check Fax Reception Image] key

   The received data is listed.

   You can also display the received data list by tapping the job status display and tapping the [Check Received Data] key on the action panel of Job Status screen.

2. #### Tap the key of the received data you wish to forward, and tap the [Forward to Other Address] key

   - Tap to show a list of received data. The list view or thumbnails view can be changed depending on the setting mode.
   - Multiple sets of received data can be selected.

   - When you select a single received data only, you can tap the [Check Image] key on the action panel and check the image on the preview screen.
   - To store the sender fax number as a number for "Allow/Reject Number Setting", tap the [Store to Unwanted Fax] key and, in the confirmation message screen, tap the [Store] key.
     Specify a sender fax number as a number for "Allow/Reject Number Setting" by selecting, in "Setting mode (administrator)", select [System Settings] → [Image Send Settings] → [Fax Settings] → [Receive Settings] → [Allow/Reject Number Setting].

3. #### Select the destination from the Address Book screen, and tap the [Start] key

Back to top