# UPPER SIDE

This section describes the names and functions of the respective parts inside the machine.
×
Toner cartridge
This cartridge contains toner. When the toner in a cartridge runs out, replace with new one.
- REPLACEMENT OF TONER CARTRIDGE
×
Fusing unit
Heat is applied here to fuse the transferred image onto the paper.
The fusing unit is hot. Take care not to burn yourself when removing a misfeed.
×
Transfer belt
This belt takes the image formed with toner off the photoconductive unit and transfers the image onto paper.
Do not touch or damage the transfer belt.
This may cause a defective image.
×
Right side cover
Open this cover to remove a misfeed.
×
Paper reversing section cover
This unit is used for reversing paper when 2-sided printing is performed. Open this cover to remove a paper misfeed.
×
Main power switch
Use this switch to turn on the power for the machine.
When using the fax or Internet fax functions, always keep this switch in the "" position.
- TURNING ON THE POWER
×
Toner collection container
This box collects excess toner that remains after printing.
- REPLACING THE TONER COLLECTION CONTAINER
A service technician collects replaced the toner collection container.
×
Toner collection container release lever
Operate this lever when you need to release the toner collection container lock to replace the toner collection container or clean the laser unit.
- CLEANING THE LASER UNIT
- REPLACING THE TONER COLLECTION CONTAINER
×
Handle
Pull this out and grasp it when moving the machine.
×
Paper drawer right side cover
Open this cover to remove a paper misfeed in tray 2, 3 or 4.
×
Right side cover
Open this to remove a paper misfeed in tray 1.
×
Right side cover release lever
To remove a paper misfeed, pull and hold this lever up to open the right side cover.
Tap the name to make its details pop up.
Back to top