# FAX DEST. CONFIRMATION MODE

This mode displays a destination confirmation message when a fax is sent to prevent accidental transmission to the wrong destination. Set it in setting mode. If a fax is sent while this function is enabled, an address confirmation message will appear when the [Start] key is tapped.
The message that appears will vary depending on the method used to specify the destination.
After tapping the [Speaker] key while "Fax Dest. Confirmation Mode" is enabled, the destination cannot be specified using the numeric keys, one-touch key, [Call Search Number] key, or [Select among addresses recently sent to] key. However, it is possible to send through a telephone.

- To display the destination confirmation message prior to fax transmission:
  In "Setting mode", select [System Settings]→[Image Send Settings]→[Fax Settings]→[Default Settings]→[Fax Dest. Confirmation Mode].
- To disable fax broadcast when Fax Dest. Confirmation Mode is enabled:
  In "Setting mode", select [System Settings]→[Image Send Settings]→[Fax Settings]→[Send Settings]→[Disable Fax Broadcasting].

Destination specified by one-touch key/search number
Tap the [Start] key to display all destinations in the destination confirmation screen. Check that the destinations are correct, and tap the [Send Confirmation] key to start scanning of the original.
If the destination is not correct, tap the [Cancel] key and select the destination again.

- You can select multiple one-touch keys for contacts or groups including fax destinations.
- Before tapping the [Send Confirmation] key, you can change scan or other settings.

Destination specified using the numeric keys, [Select among addresses recently sent to] key, or [Global Address Search] key
Tap the [Start] key to display the confirmation message.
Tap the [OK] key, re-enter the destination using the numeric keys, and tap the [Send Confirmation] key.
If the re-entered destination is correct, scanning will begin.
If the re-entered destination is not correct, a message will appear. Tap the [OK] key and re-enter the destination. If an incorrect address is entered three times for confirmation, all the previous settings are cancelled, and you will return to the base screen.

- You can use the numeric keys to enter fax numbers serially. In that case, tap to enter the destination fax number to be added.
- If the [Sub Address] key was tapped to enter a sub-address and passcode, the fax number must be re-entered during confirmation. After re-entering the fax number, tap the [Sub Address] key and enter the sub-address and passcode.
- If chain dialling was used, tap the [Pause] key to enter "-" during confirmation.
- Before tapping the [Send Confirmation] key, you can change scan or other settings.

When a fax that was selected from the addresses sent recently has been resent
A confirmation screen is displayed based on the method used to specify the destination during the previous transmission.
Back to top