# AUTO COLOUR CALIBRATION

Settings related to the printer function can be configured.
Performs automatic colour correction when the colour in colour copies is off.
The machine prints a test patch, the test patch is scanned, and the colour is automatically corrected.
After the [Execute] key is tapped and a test patch is printed, a message appears prompting you to begin automatic calibration.
Place the test patch on the document glass as shown below (so that the thin line at the edge of the page is to the left).
Lay copy paper (about five sheets) that is the same size as the test patch on top of the placed test patch, gently close the automatic document feeder, and tap the [Execute] key.

- Before executing Auto Colour Calibration, check to see if the registration adjustment is correct.
  If the registration adjustment is not correct, perform "Registration Adjustment."
- If the colour is still off after performing Auto Colour Calibration, repeating Auto Colour Calibration once again may improve the colour.

Back to top