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Active 
Collaboration Soundbar

SP-ASCM
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Parallelperspektive möglich?
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Collaborative Soundbar including 2x USB-Cable + power supply
Wallmount
4x M3 Screws + washers
2) Assembly to the wall
1) Delivery

3) Connection


 
Camera USB (3.0)			USB port 2.0 of the external device 
Microphone USB (2.0)			USB port 2.0 of the external device 	

4) Devices

[bookmark: _GoBack]
Playback device						“2 – Phnx MT103_16k”
Recording device					“2 – Phnx MT103_16k”
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Use level to mark
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Drill holes (4x)
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