# TONER DOES NOT ADHERE WELL OR CREASES APPEAR ON THE PAPER

Point to check | Solution
--- | ---
Are you using paper that is not within the specifications? | Use SHARP-recommended paper. Using paper that is for other models or special paper that is not supported may result in misfeeds, creases, or smudges. - "SUPPLIES" in "Quick Start Guide"
Has the paper type been set correctly? | Set the correct paper type in the tray settings. Make sure that the following has not occurred: Heavy paper is being used, but a paper type other than heavy paper is selected in the tray settings. (The image may disappear if rubbed.) Paper other than heavy paper is being used, but heavy paper is selected in the tray settings. (This may cause creases and misfeeds.) "Setting mode" → [Paper Tray Settings]→[Tray Registration]
Is the paper loaded so that printing takes place on the reverse side? | Check the front and reverse side of paper. Some types of paper such as labels and transparency films have specific front or reverse sides. If printing takes place on the wrong side of label sheets or transparency film, the toner may not adhere well and a clear image may not be obtained.

Back to top