# PAPER FEEDING IN A MACINTOSH ENVIRONMENT

This section explains the [Paper Feed] settings in the print settings window.

- When [Auto Select] is selected:

- A tray that is set for plain or recycled paper (only plain paper in the factory default setting) of the size specified in "Paper Size" on the page setup screen is automatically selected.

- When a paper tray is specified:

- The specified tray is used for printing regardless of the "Paper Size" setting on the page setup screen.
  For the bypass tray, also specify the paper type. Check that the paper type that is set for the bypass tray of the machine, check that paper of that type is actually loaded into the bypass tray, and then select the appropriate bypass tray (paper type).

- When a paper type is specified:

- A tray with the specified type of paper and the size specified in "Paper Size" on the page setup screen is used for printing.

Special media such as envelopes can also be placed in the bypass tray.
For the procedure for loading paper in the bypass tray, see "LOADING PAPER INTO THE BYPASS TRAY".
When [Enable Detected Paper Size in Bypass Tray] (disabled by factory default) or [Enable Selected Paper Type in Bypass Tray] (enabled by factory default), which you can reach by selecting [System Settings] in "Setting mode" → [Printer Settings]→[Default Settings]→[Bypass Tray Settings] is enabled, printing will not take place if the paper size or paper type specified in the printer driver is different from the paper size or paper type specified in the settings of the bypass tray.
To exclude the bypass tray from the trays that can be selected when [Auto Select] is selected:
In "Setting mode", select [System Settings]→[Printer Settings]→[Default Settings]→[Bypass Tray Settings]→[Exclude Bypass-Tray from Auto Paper Select].
Back to top