# ADDING MARGINS(MARGIN SHIFT)

## Overview

This function shifts the copy image right, left or down to adjust the margin.
This is convenient when you wish to bind the copies with a string or in a binder.
Shifting the image to the right so the copies can be bound at the left edge

Not using the Margin Shift | Using the Margin Shift
--- | ---

Staple positions
Rotation copy cannot be used in combination with the margin shift function.
To change the default margin shift setting:
In "Setting mode", select [System Settings]→[Copy Settings]→[Copy Setting]→[Initial Margin Shift Setting].

## Operation

Place the original and tap the [Preview] key.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Tap the [Others] key, and tap the [Margin Shift] key.
Tap the image shift direction.
Sets a margin shift width.

- Tap the numeric value display indicating the margin shift area on the front side or reverse side, and enter the area using the numeric keys.
- To quickly set the area, first specify a value close to the desired value by the numeric keys, then adjust it with .
- If you set the [Adjust 2nd pg value to 1st.] checkbox to , goes out and you can set sides 1 and 2 separately.

After the settings are completed, tap and [Back] keys in sequence.

- To cancel the margin shift setting:
  Tap the [Off] key.
- To cancel all settings:
  Tap the [CA] key.

Check the preview image in the preview screen.
Check whether or not settings produce the required results.
To cancel all settings:
Tap the [CA] key.
Tap the [Colour Start] or [B/W Start] key to start copying.
When making only one set of copies, you do not need to specify the number of copies.
To make two or more sets of copies:
Tap the copies display key to specify the number of copies.
Back to top