# AUTOMATIC ADJUSTMENT OF EXPOSURE AND ORIGINAL TYPE

Automatic exposure adjustment operates by default to automatically adjust the exposure level and original type as appropriate for the original being copied. ("Auto" is displayed.)
This function automatically adjusts the image during black & white copying and full colour copying to obtain the most suitable copy.

- To change the default exposure:
  In "Setting mode", select [System Settings]→[Copy Settings]→[Initial Status Settings]→[Exposure Type].
- To adjust the exposure level when [Auto] is used for the copy exposure:
  In "Setting mode", select [System Settings]→[Copy Settings]→[Copy Setting]→[Copy Exposure Adjustment].

Back to top