# ADJUSTING THE COLOUR(COLOUR BALANCE)

## Overview

This function adjusts the colour, tone, and density.
This function divides each of colours, yellow, magenta, cyan, and black, into eight gradations from light to dark, and adjusts the average density of each gradation.
As necessary, it collectively adjusts all eight gradations.
Colour Balance must be specified before scanning the original.
To change the default colour balance setting:
In "Setting mode", select [System Settings]→[Copy Settings]→[Colour Adjust]→[Initial Colour Balance Setting].

## Operation

Tap the [Others] key, and tap the [Colour Balance] key.
Tap the tab of the colour you want to adjust.
Tap the key or slide the slider to adjust the colour balance.
To individually adjust eight sliders, set the [Set in a Batch] checkbox to , and slide the control of each slider.
When using the key to individually adjust eight sliders, tap the required slider and tap the key.
As necessary, tap the tab of each colour, and repeat this step.
Colour Balance Setting

- To return the current colour balance to the default:

- Tap the [Size Reset] key.

- To return all colour balances to defaults:

- Tap the [Cancel All] key. The values of all eight gradations will return to the default colour balance values.
  The default colour balance is set by selection of [System Settings] in "Setting mode" →[Copy Settings]→[Colour Adjust]→[Initial Colour Balance Setting].

Place the original and tap the [Preview] key.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Tap the [Colour Start] key to start copying.
When making only one set of copies, you do not need to specify the number of copies.
To make two or more sets of copies:
Tap the copies display key to specify the number of copies.
Back to top