# INITIAL STATUS SETTINGS

The following settings are related to copying.
Default settings selected with these settings apply to all functions of the machine (not just the copy function).
The copier settings are reset to the initial state when the [Power] button is turned on, when the [CA] key is tapped, or when the auto clear interval has elapsed. These settings are used to change the default settings for copy mode.
The following settings can be changed:

Item | Description
--- | ---
Colour Mode | Configure default colour mode settings.
Paper Tray | Specify the paper tray that is selected by default.
Exposure Type | Configure default exposure mode settings.
Copy Ratio | Specify the copy ratio that is selected by default.
2-Sided Copy | Configure the 2-sided mode settings that are selected by default. If this setting is used to change the default setting for the duplex function to any setting other than "1-Side to 1-Side" and the duplex function or automatic document feeder fails or is disabled, the setting will revert to "1-Side to 1-Side".
Output | Set the print output method and output tray that are selected by default.
Offset | Set whether or not offset is performed in the default settings.
Return to the Defaults | This returns all items to the factory default settings.

Back to top