# EXTERIOR

This section describes the names and functions of the respective parts on the exterior of the machine.
×
Automatic document feeder
This automatically feeds and scans multiple originals. Both sides of 2-sided originals can be automatically scanned at one time.
- AUTOMATIC DOCUMENT FEEDER
×
Front cover
Open this cover to switch the main power switch to "On" or "Off" or to replace a toner cartridge.
- TURNING ON THE POWER
- REPLACEMENT OF TONER CARTRIDGE
×
Output tray (centre tray)*
Printed paper is output into this tray.
×
Operation panel
This panel hosts the [Power] button, [Power Save] button/indicator, [Home Screen] button, main power button and touch panel. Use the touch panel to operate each of these functions.
- OPERATION PANEL
×
Right tray*
Set so that paper is output into this tray as required. By setting originals received via fax or Internet fax to be output into this tray, you can separate them from paper output from copying.
×
Finisher*
This staples paper.
A punch module can also be installed to punch holes in output paper.
- FINISHER
×
Saddle finisher*
This staples and folds paper. A punch module can also be installed to punch holes in output paper.
- SADDLE FINISHER
×
Paper pass unit*
This unit relays between the machine and the saddle finisher by sending printed paper to the saddle finisher.
×
USB port (A type)
This is used to connect a USB device such as a USB memory device to the machine.
For the USB cable, use a shielded cable.
Supports USB 2.0 (Hi-Speed).
×
Keyboard
Use this as a substitute for the soft keyboard displayed on the touch panel. When not being used, it can be stored under the operation panel.
×
Tray 1
Store paper in this tray.
- LOADING PAPER INTO A TRAY
×
Tray 2*
Store paper in this tray.
- LOADING PAPER INTO A TRAY
×
Tray 3*
Store paper in this tray.
- LOADING PAPER INTO A TRAY
×
Tray 3*
Store paper in this tray.
- TRAY 3 - 4 (STAND/500&2000 SHEET PAPER DRAWER)
×
Tray 4*
Store paper in this tray.
- LOADING PAPER INTO A TRAY
×
Tray 4*
Store paper in this tray.
- TRAY 3 - 4 (STAND/500&2000 SHEET PAPER DRAWER)
×
Tray 5 (MX-LC11)*
Store paper in this tray.
- LOADING PAPER INTO A LARGE CAPACITY TRAY
×
Bypass tray
Use this tray to feed paper manually.
When loading paper larger than A4R or 8-1/2" x 11"R, pull out the extension guide.
- LOADING PAPER INTO THE BYPASS TRAY
Tap the name to make its details pop up.
* Optional Back to top