# REPLACING THE TONER COLLECTION CONTAINER

## Overview

The toner collection container collects excess toner that is produced during printing. When the toner collection container becomes full, "Replace used toner container." will appear.

- Do not throw the toner collection container into a fire. Toner may fly and cause burns.
- Store the toner collection container out of the reach of small children.

## Operation

Open the front cover.
Move the toner collection container lock to the release position to have the toner collection container fall forward until it stops.
Keep the replacement cleaner that has not been used.
Store it at the left of the new toner collection container.
Remove the toner collection container.
Hold the toner collection container by both hands and lift it up slowly.
Place the toner collection container on a flat surface.
Place a sheet of paper such as newspaper on the surface before placing the toner collection container.

- Do not point the holes down as used toner will spill out.
- Keep the toner collection container you have removed in a plastic bag (do not discard them). Your service technician will collect them.

Install a new toner collection container.
Insert the box from above at a slant. (In the direction opposite to the direction you removed it in.)
Push the toner collection container into the machine.
Push the box in until it clicks into place.
Lock the toner collection container.
Move the toner collection container lock to the lock position.
Close the front cover.
Back to top