# CLEANING THE MAIN CHARGER OF THE PHOTOCONDUCTIVE DRUM

## Overview

If black lines or coloured lines appear even after you have cleaned the document glass and automatic document feeder, use the charger cleaner to clean the main charger that charges the photoconductive drum.

- If cleaning the main charger of the photoconductive drum does not solve the problem, pull the knob out and push it back three more times.
- When pulling and pushing the knob to clean the charger, pull and push the knob slowly from one end to the other.

## Operation

Open the front cover.
Move the lock of the toner collection container to the release position, push it down until the toner collection container stops, and then slowly lift it up to remove it.
Remove the charger cleaner.
The charger cleaner is attached to the front cover of the machine.

1. Press on the right-hand side of the charger cleaner to put it off the hook.
2. Bring it over the hook to place it near side.
3. Around boss (A), rotate the charger cleaner to put it off the hook on the left.

Clean the main charger.
Gently push the charger cleaner all the way in, and gently pull it out.
Insert it so that label (A) on the cleaning target side and label (B) on the charger cleaner side are oriented as shown.
Repeat step 4 with all other main chargers.
There are a total of 4 places to be cleaned in the machine as shown.
Replace the charger cleaner in its original position.

1. Engage the charger cleaner onto boss (A) to rotate it, and then put the tip (the side without a handle) on the hook on the left.
2. Put the right-hand side of the charger cleaner over the hook to place it in the back.
3. Put the charger cleaner on the hook.

Install a toner collection container.
Insert the box from above at a slant. (In the direction opposite to the direction you removed it in.)
Push the toner collection container into the machine.
Push the box in until it clicks into place.
Lock the toner collection container.
Move the toner collection container lock to the lock position.
Close the front cover.
Back to top