# DEFAULT SETTINGS

Settings related to the printer function can be configured.
Printer condition settings are described below.
Prohibit Notice Page Printing
Disables to print a notice page.
Prohibit Test Page Printing
Disables to print the test page.
When this setting is enabled, [System Settings]→[List Print (User)]→[Printer Test Page] in "Setting mode" cannot be used to print test pages.
A4/Letter Size Auto Change
When printing an 8-1/2" x 11" (A4) size image, this setting allows A4 (8-1/2" x 11") size paper to be used if 8-1/2" x 11" (A4) size paper is not loaded.
Print Density Level
This lightens or darkens the print density of colour and black and white images. The print density can be adjusted to five levels.
CMYK Exposure Adjustment
Adjusts the density of cyan (C), magenta (M), Yellow (Y), and Black (K). The exposure of each colour can be adjusted to 17 levels.
Bypass Tray Settings
Enable Detected Paper Size in Bypass Tray
This is used to prohibit printing when the paper size specified for a print job is different from the paper size inserted in the bypass tray.
Enable Selected Paper Type in Bypass Tray
This is used to prohibit printing when the paper size specified for a print job is different from the paper size inserted in the bypass tray.
Exclude Bypass-Tray from Auto Paper Select
When [Auto] is selected for paper type selection, the bypass tray is excluded from the trays that can be selected. This is recommended when special paper is often placed in the bypass tray.
Job Spool Queuing
When this function is enabled, received print jobs are displayed in the spool queue of the job status screen. The jobs are moved to the job queue after they have been analyzed by the machine. Multiple jobs that have not yet been analyzed appear in the spool queue.
When this function is disabled, received print jobs are displayed in the job queue instead of being displayed in the spool queue. However, when an encrypted PDF job is printed, the job appears in the spool queue.
Prohibit USB Memory Direct Print
Disables the function for directly printing of a file in a USB memory device.
Disabling of Network Folder Direct Print
Disables the direct printing from a network folder.
Disabling sending while printing
Disables the Image Send function during printing.
Back to top